HOME :: SITE MAP :: CONTACT
d s l s e t u p 1 Instructions for setting up DSL in Windows 95/98 Installing network card into your computer. Connecting the DSL line to you computer. Setting up your computer to use the DSL line. Setting your Programs to connect using the DSL line. Other Steps: Installing the CA-CONNECT Software • Troubleshooting • Complete List of Settings You should have a steady power LED on the modem and a steady DSL LED (not blinking), If you have a blinking DSL LED, Please call CascadeAccess. The LAN LED may or may not be on solid (if your is off it will be off). If everything is working properly you will have the first 3 LEDS (from left to right) on solid. If not, no need to go any further. These instructions assume your DSL is hooked up and your Network Card is installed and working. CascadeAccess uses a Infinlink i500 DSL Modem. This modem has no user changeable settings. We support the G.Lite ITU G.992.2 standard thus a G.992.2 compliant modem should work with our DSL service. We can support PPPoE (RFC 2516) or PPPoA (RFC 2364) standards. These instructions are for the PPPoE installation. Installing network card into your computer. » If you currently have a network card skip to step 2. » To install your network card, follow the directions that came with the card. ::top:: Connecting the DSL line to you computer. » Plug the Ethernet cable that came with the DSL modem into network card » Plug the other end of the Ethernet cable into the port on the modem labeled LAN » If you have multiple computers with a hub you would need to plug the one end of the Ethernet cable into the hub and the other into the port labeled LAN on the back of the DSL modem (a crossover cable may be required) » Take the phone cord that came with the modem and plug the end into the phone jack. Take the other end and plug it into the port on the modem labeled DSL » Take the Power cord and plug it into the back of the DSL modem » Take the other end of the power cord and plug it into a power outlet ::top:: Setting up your computer to use the DSL line. » On your Desktop click on “Start” » Click on “Settings” » Click on “Control Panel” » Double Click on the Icon labeled “Network” » Click on the identification tab and write down the computer name (we will use this later) » Click back to the configuration tab and in the box scroll down until you see TCP/IP » There might be a few of them. Click on the one that says just “TCP/IP” or the one that says “TCP/IP ŕ Ethernet Adapter”. (Ethernet Adapter is the name of you network card installed into you computer) » Click on “Properties” » Click on “IP Address” » Enter "192.168.0.2" in the field labeled IP address » Enter "255.255.255.0" in the field labeled Subnet Mask » Click on the “DNS Configuration” tab » Enter in the name of your machine (you wrote this down earlier) in the field labeled "Host” » Enter “cascadeaccess.com” in the field labeled “Domain” » Enter “64.233.104.2” in the field labeled “DNS Server Search order” » Click “Add” » Enter "205.238.26.97" in the same field labeled “DNS Server Search order” »Click “Add” » Enter “cascadeaccess.com” in the field labeled “Domain Suffix Search Order” »Click “Add” » Click “OK” » Click “OK” again » Your computer might ask you for the windows 95/98 CD and copy some files » Your computer will ask you to restart - say “YES” » When your computer restarts the configuration is complete ::top:: Setting your Programs to connect using the DSL line. » Click on “Start” » Click on “Settings” » Click on “Control panel” » Click on the Icon labeled “Internet Options” » Click on the tab labeled “Connections” » Click on the circle next to “Never dial a connection” So there is a dot in it » Click on the button labeled “LAN Settings” » Click in the box next to “Automatically detect settings” so there is a check in it » Click “OK” » Click “OK” again » Close the “Control Panel” » You are now ready to install the CA-Connect Software ::top:: Next Step: Installing the CA-CONNECT Software |
| o u r s e r v i c e s We offer a variety of packages and services to suit your needs.
| t e c h s u p p o r t We provide customer service 24 hrs/7days a week.
| n e t g u i d e s Guides to the Web for both 'newbies' and 'techies'.
| o u r c o m m u n i t y Find our more about the communities Cascade Access serves.
| o r d e r f o r m Ready to order? Use our online ordering form to get started.
| o u r f a q s Click here for frequently asked questions about our services.
Privacy Policy :: Disclaimer Copyright © 2002 Cascade Access. All rights reserved. To report problems with this site, please email the webdiva@fluidcommunications.biz
o u r s e r v i c e s | t e c h s u p p o r t | n e t g u i d e s | o u r c o m m u n i t y | o r d e r f o r m | o u r f a q s